{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["电子元器件"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"电子元器件","index":0,"n_rows":199,"n_cols":6,"rows_kept":199,"cut":false,"hidden":false,"merged":[]}
["名称","规格","盒子编号","LC商城编号","库存"]
["电容","0603-10nF-50V-10% | 0402-50v",1,"C60133","80|100"]
["电阻","0603-15K-100mw-1% | 0201 | 0402",2,"C22809","90|100|100"]
["电阻","0603-1K-100mw-1% | 0201|0402",3,"C144087","70|100|100"]
["电阻","0603-22Ω-100mw-1%",4,"C23345",80]
["电阻","0603-8.2K-100mw-1%",5,"C25981",90]
["电阻","0805-91K-100mw-1%",6,null,90]
["点位器","插件-200K-10%",7,"C118922",3]
["电阻","0603-37.4K-100mw-1% | 0402",8,"C185422","85|100"]
["电阻","0603-80.6K-100mw-1%",9,"C245172",70]
["电阻","2512-10mΩ-3w-1%",10,"C2994644",9]
["电容","0603-2.2NF-50V-5% | 0402",11,"C106861","45|100"]
["肖特基二极管","SMA-40v-5A-SS54",12,"C22452",10]
["电阻","0603-3K-100mw-1%",13,"C125893",80]
["电阻","0805-11K-100mw-1%",14,null,70]
["电容","0805-10UF-25V-10%",15,"C15850",25]
["电阻","0603-12K-100mw-1%",16,"C22790",170]
["电阻","0603-41.2K-100mw-1% | 0201",17,"C321898","165|100"]
["电阻","0603-2K-100mw-1%",18,null,50]
["场效应管","N沟道-60V-115MA-SOT-323（SC-70）",19,"C190607",17]
[null,"CH224K",20,null,3]
["AD采集","PCF8591T",21,null,5]
["热敏电阻","PT-100",22,null,5]
[null,"8H3K32S2",23,null,3]
["MOS管","FDD8896-252",24,"C10867",11]
["三极管","SS8050-H-SOT-23-3L",25,"C699255",2]
["电感","7.4*6.6*3-15UH-115mΩ-2.6A",26,"C3002640",5]
[null,"NR252012-2R2M",27,null,15]
["轻触开关","2*4*3.5-SMD",28,"C692458",10]
["超级电容","SMD-4.8*1.4-70000UF-3.3V",29,"C396469",4]
["电位器","SMD-200K-25%",30,"C128551",6]
["固态继电器","221G2-40V",31,null,4]
["电阻","0402-330K-62.5mw-1%",32,"C25778",100]
["GPS","ATGM332D-5N31-SMD",33,"C128659",2]
["按键开关","插件",34,"C963201",1]
["Type-C","母座-SMD",35,"C709028",3]
["电容","0603-2.2UF-16V-10%",36,"C914769",1]
["电容","0805-22UF-50V-10%|0402-6.3V_20%",37,"C415703","90|10"]
["二极管","SS510-100V",38,"C2898359",10]
["TVS","单向-5V-SMB",39,null,9]
["电阻","0603-10K-100mw-1% | 0201|0402",40,"C25804","150|100|100"]
["肖特基二极管","SMA-40V-2A",41,"C908678",35]
["GPS","ATGM336H-5N31",42,"C90770",1]
["线性稳压器","SOT-223-LP1116-15G3F",43,"C2935094",3]
["TVS/ESD-静电保护","0402-双向TVS-5V-3A",44,"C316041",38]
["TVS","单向-5V-DFN1610-2",45,"C172440",8]
["肖特基二极管","SMA-40V-3A",46,"C2891718",19]
["自恢复保险丝","1206-2A",47,"C20988",5]
["自恢复保险丝","1210-3A-6V",48,"C70183",2]
["电位器","插件-500K-10%-3296",49,"C118920",6]
["开关二极管","SOD-123-100V-150MA-8NS",50,"C84367",95]
["MOS管","NCE60P50K",51,"C130104",17]
["LED","绿-0603",52,"C72043",8]
["电平移位器","TSS0P-20-RS0108YQ20",53,"C2762289",3]
["RF射频连接器","IPEX-内针-SMD",54,"C2894919",14]
["射频低噪声放大器","AT2659-DFN-6",55,"C92450",4]
["场效应管","N沟道-60V-50A-TO-252-2",56,"C96013",5]
["电容","0603-33PF-50V-5% | 0201 | 0402-1%",57,"C1663","50|100|100"]
["LED","红-0603",58,"C72044",40]
["采样电阻","2512-100mΩ-3w-1%",59,"C393067",30]
["电感","0201-6.8NH-3%-620mΩ",60,"C76757",90]
["电阻","0603-42.2K-100mw-1%",61,"C23167",60]
["电阻","0603-470Ω-100mw-1%",62,"C23179",75]
["电阻","0603-4.7K-100mw-5%",63,"C144596",55]
["电阻","0603-33K-100mw-5%",64,"C101331",65]
["电容","0603-150PF-200V-5%",65,"C63701",18]
["铝电解电容","SMD-10UF-50V-5*1.5",66,"C2992603",16]
["稳压器","SMD-3.3V-LP1116",67,null,5]
["电源芯片","MP2451DT-3.3~5V",68,null,5]
["PWM","PCA9685",69,null,2]
["电感","0805-6.8NH-5%-110mΩ-1.73*2.29",70,"C186946",3]
["稳压器","SMD-3.3V-78M05",71,null,2]
["电源芯片","MP1584EN-3.3~5V",72,null,4]
["电容","0603-10PF-50V-5%",73,null,70]
["电容","0603-22PF-50V-5%|0402-1%",74,"C277482","70|100"]
["铝电解电容","SMD-220UF-50V-10*10.5",75,null,4]
["铝电解电容","SMD-220UF-50V-10*10.5",76,null,1]
["电阻","0603-240K-100mw-5%",77,"C245197",70]
["铝电解电容","SMD-47UF-16V-5*5.4",78,"C336193",20]
["铝电解电容","SMD-100UF-16V-6.3*5.4",79,"C5361259",20]
["电阻","0603-0Ω-10w-1% | 0201 | 0402",80,"C21189","160|100|100"]
["电阻","0805-24K-125mw-1%",81,"C228659",60]
["电阻","0805-75K-125mw-1%",82,"C137491",55]
["电容","0603-470PF-50V-5%",83,"C106211",60]
["接线端子","1*2",null,null,7]
["USB2","直插-公-2CM",null,null,9]
["USB2","弯插-母",null,"C86461",4]
["尖头探针","P100-3.5",null,null,10]
["排针","1*40",null,null,18]
["排母","2*20",null,null,6]
["按键开关","插件-DPST",null,"C309202",10]
["USB3","母-弯插",null,"C381137",9]
["USB3","公-夹板式",null,null,10]
["铝电解电容","直插-10UF-100V-20%-6.3*11",null,"C2029",19]
["子弹头套","公-母-壳",null,null,90]
["miniPcie","52p-5.2H",null,null,2]
["拨码开关",null,84,null,4]
["继电器","直插-松下",85,null,3]
["铝电解电容","直插-220UF-100V-20%",null,null,3]
["同轴连接器","SMA-内孔",null,null,25]
["USB2","直插-公-1.5CM",null,null,4]
["继电器","直插-Y3F-SS-112D",null,null,8]
["开关二极管","插针-75V-200ma-4ns",null,"C14516",45]
["电流感应放大器","INA226AIDGSR-MSOP",173,"C49851",1]
["电源芯片DC-DC","TPS54332DDAR-SOP-8-EP",86,"C41312",1]
["电源管理芯片-DC","TPS65251RHAR-VQFN-40-6*6",87,"C60246",1]
["肖特基二极管","SMA-20V-3A-B320A-13-F",88,"C110484",4]
["无源晶振","SMD3225-4p-25MHZ-10PPM-12pf",89,"C91750",4]
["TVS/ESD-静电保护","DFN-10L-双向TVS-5V-3.5A",90,"C316044",8]
["TVS/ESD-静电保护","DFN1006-ESDA33CP",91,"C384838",5]
["肖特基二极管","SOD-123-20V-500MA",92,"C91741",4]
["无源晶振","SMD3225-4p-24MHZ-10PPM-12pf",93,"C70590",10]
["电阻","0603-75K-100mw-1% | 0201 ",94,"C23242","90|100"]
["电容","0603-180PF-50V-1% | 0201-25V-10% | 0402-50V-5%",95,"C527047","45|100|100"]
["电容","0603-10PF-50V-1%|0402",96,"C309467","43|100"]
["电容","0603-15NF-25V-5% | 0402",97,"C519541","90|100"]
["电阻","0603-1MΩ-100mw-1% | 0201",98,"C22935","95|100"]
["电阻","0603-2MΩ-100mw-1%",99,"C22976",95]
["电阻","0603-100Ω-100mw-1%",100,"C105588",95]
["电容","0603-3.3uF-25V-10% | 0402-10V",101,"C342962","9|15"]
["电阻","0603-383K-100mw-1% | 0201 | 0402",102,"C2933214","95|100|100"]
["电阻","0603-12.4K-100mw-1% | 0201 |0402",103,"C269455","94|40|100"]
["电容","0603-12pF-50V-5% | 0201 | 0402-1%",104,"C38523","93|100|100"]
["磁珠","0603-2.5K-100MHZ-单路",105,"C77668",45]
["电阻","0603-48.7K-100mw-1% | 0201",106,"C23063","95|100"]
["钽电容","CASE-3528-10uF-25V-10%",107,"C161582",10]
["电感","SMD-4.7UH-20%-5.5A-38mΩ-6.6*7.1*3",108,"C207840",12]
["电阻","0603-120K-100mw-1% | 0201",109,"C25808","95|100"]
["电阻","0603-100K-100mw-1% | 0201|0402",110,"C116674","39|100|100"]
["电容","0805-47uF-10V-20%",111,"C386058",2]
["电阻","0603-7.5K-100mw-1% | 0201",112,"C365451","40|100"]
["电源芯片DC-DC","TPS54531DDAR-SOP-8-EP",114,"C50605",10]
["STC-51芯片","STC15W104-35I-SOP8",113,"C56492",1]
["miniPcie","6.7H-52P",null,null,2]
["HDMI","SMD-母-19P",115,"C400326",3]
["板对板连接器","SMD-100P-0.4MM-H3.0-母",116,"C19274168",6]
["板对板连接器","SMD-100P-0.4MM-公",117,"C531031",3]
["电阻","0603-10Ω-100mw-1% | 0201|0402",118,"C22859","100 |100|100"]
["钽电容","CASE-6032-220UF-10V-10%",119,"C122293",3]
["电阻","0603-12.7k-100mw-1% | 0201|0402",120,"C269456","100|100|100"]
["电感","SMD-2.5UH-20%-12A-7*6.6-0630",121,"C2453297",1]
["电阻","0603-20K-100mw-1% | 0201 | 0805-125mw | 0402-62.5mw",122,"C4183","95|100|70|100"]
["电容","0603-10uF-10V-10% | 0402-20%-10v",123,"C19702","95|70"]
["采样电阻","2512-2MΩ-3w-1%",124,"C2994640",28]
["SiM卡连接器","SMD-翻盖-nano-6P",125,"C77877",2]
["电容","0603-47nF-50V-10% |  0201-25V | 0402-5%-50v",126,"C1622","95|100|100"]
["电容","0603-4.7nF-50V-10% | 0201 | 0402-5%",127,"C53987","90|100|100"]
["电容","0603-10uF-25V-10%",128,"C344022",19]
["电容","0603-100nF-50V-10% | 0201 | 0402-5%-25V",129,"C1591","66|100|100"]
["电阻","0603-150K-100mw-1% | 0201",130,"C114660","95|100"]
["电阻","0603-130K-100mw-1% | 0201 | 0402",131,"C22795","95|100|30"]
["电容","0603-0.1nF-25V-10%",132,null,40]
["电阻","0603-40.2K-100mw-1% | 0201 | 0402",133,"C12447","95|100|100"]
["钽电容","CASE-3528-100uF-10V-20%",134,"C126471",4]
["钽电容","CASE-2.5*3.5-22uF-20V-10%",135,"C2976914",2]
["电容","0603-1uF-50V-10% | 0201 | 0805-50v | 0402-25v",136,"C15849","94|100|15|100"]
["电阻","0201-1.5K-50mw-1% | 0402",137,"C304512","100|100"]
["电容","0603-100pF-50V-5% | 0201 | 0402-1%",138,"C1635","60|100|100"]
["电容","0603-4.7pF-50V-5%",139,"C29823",7]
["插头","XT30-M-公头",140,"C431092",3]
["功率电感","0420-4.7UH-SMD,4.05x4.45x2mm",141,"C436517",7]
["USB拓展芯片","VL822-QFN76",142,"C2841047",1]
["XT30转XT60","XT30-公 转 XT60 母",null,null,4]
["XT30转XT60","XT30-母 转 XT60 公",null,null,4]
["miniPcie","52p-90H",null,null,5]
["采样电阻","0805-2MΩ-500mw-1%",143,"C163090",10]
["电容","0201-100pF-25V-5%",144,"C389108",100]
["电容","0201-10pF-25V-5%",145,"C541202",100]
["电容","0402-4.7uF-25V-5% | 0805-10%-50v",146,"C2858031","20|10"]
["电阻","0402-10.2K-62.5mw-1%",147,"C226746",100]
["电感","SMD-4.7UH-20%-9A-6.6*7",148,"C167220",5]
["电感","SMD-4.7UH-20%-3.5A-4.5*4.1",149,"C436517",5]
["磁珠","0603-600Ω-100MHZ-单路",150,"C19330",100]
["电容","0402-100nf-5%-50V",151,"C131394",100]
["电阻","0402-51.1k-1%",152,"C25904",100]
["功率电子开关","SOT-23-5-STMPS2151STR",153,"C135998",2]
["电阻","0402-1.96k-1%",154,"C170254",50]
["电阻","0402-82k-1%",155,"C137932",100]
["肖特基二极管","SMC-B540C-40V-5A",156,"C72264",5]
["功率电感","SMD-5.6UH-6A",157,"C128689",5]
["电阻","0402-38.3k-1%",158,"C226710",50]
["电容","0402-1nF-50V-10%",159,"C106205",100]
["电容","0402-8.2nF-50V-10%",160,"C541457",100]
["电阻","0402-2.2k-1%",161,"C114762",100]
["板对板连接器","SMD-100P-0.4MM-母",162,"C19274168",10]
["无源晶振","12MHZ+10ppm+20pf",163,"C9002",10]
["电容","0402-22uF-10V-20%",164,"C6119813",5]
["USB转换芯片","SOP-16 SL2.1A USB2.0-HUB",165,"C192893",5]
["电阻","0402-22k-1%",167,"C82868",100]
["功率电子开关","MT9700-SOT-23-5",168,"C89855",10]
["电源芯片DC-DC","CL1652AB-SOT-23-5",169,"C2995665",5]
["功率电感","2.2uh-3.8A-20%-1008",170,"C5832372",10," "]
["电阻","0402-3.4k-1%",171,"C273342",100]
["功率电感","2.2uh-6A-20%-SMD-4*4",172,"C2926400",5]
["电源芯片DC-DC","JW5062T-SOT23-6",174,"C371421",4]
["音频编解码芯片","WM8960CGEFL/V-QFN-32-EP(5x5)",175,"C3025583",2]
["电阻","0402-140k-1%",176,"C114151",100]
["电阻","0402-30k-1%",177,"C138008",100]
["无源晶振","12MHZ+10ppm+10pf",178,"C2896601",4]